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	CSM-400-FM02 Record BIM QC Assessment Checklist


Design Agency uses this form to document their findings when conducting quality check (QC) on a project as required by Section 400 Rev. 1 and subsequent revisions.[footnoteRef:1]  Submit completed form (along with the submitted Record BIM deliverables) to LANL at end of project closeout for scoring/total score. [1:  FM02 may be used for Section 400 r0 with very minor adaptations.] 

Detailed instructions follow the checklist. For Project BIM assessment, use CSM-400-FM01.
	Section A. Record BIM Information

	Building:
	[bookmark: Text1]     
	Project Name:       

	Project Number (ESR, PID, DCF):
	     

	LANL Project Manager: 
	     

	BIM QC by:
(Project Team member name)
	     
	Date Reviewed:
	Click or tap to enter a date.

	Design Agency
	     
	TOTAL SCORE: (out of 27 for new; out of 29 for an existing building)
	     

	* Asterisk/baby blue indicates check is only required when updating an existing master BIM; N/A otherwise

	Scoring:
LANL will apply points upon review
	Scores are calculated based on “Yes”, “No” or “N/A” values.  Yes = equates to 1 point, No = no points awarded, N/A = not applicable.  Total possible points (100%) = 27 (new BIM) or 29 (existing BIM update). 
When not 100%, Design Agency must take steps to achieve same before next phase submission.
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LANL
STD-342-300, CAD Standards Manual, Section 400 BIM Standards
CSM-400-FM02-Rev. 0 (7/21/26), Record BIM QC Assessment Checklist

	[bookmark: _Hlk40246108]Section B. Project Deliverables

	
	Yes
	No
	N/A
	
	Yes
	No
	N/A
	SCORE

	1. Constructor Name:
	     

	2. Verify LANL Project BIM QC comments been reconciled
	☐
	☐
	☐
	8. Design Agency email response stating Project BIM comments were reconciled in documents folder
	☐
	☐
	☐
	     

	3. Constructor TIII redlines/Design Agency highlights & initials
	☐
	☐
	☐
	9. Date redlines received
	XX/XX/XXXX
	☐
	     

	4.  Record BIM
	☐
	☐
	☐
	10. Standards files provided
	☐
	☐
	☐
	     

	5. TIII PDFs provided
	☐
	☐
	☐
	11. Documents provided: photos, deliverable notifications, PEL files (excel), BIM QC form, etc.
	☐
	☐
	☐
	     

	6. -NEW groups provided*
	☐
	☐
	☐
	12. -R Removals groups provided*
	☐
	☐
	☐
	     

	7. Redlines incorporated
	☐
	☐
	☐
	
	
	
	
	



Comments:
Assessor comments should be black and responses from design team in red.
	







	Section C. Record BIMs (Model Content)

	
	Yes
	No
	N/A
	
	Yes
	No
	N/A
	SCORE

	Template Version
	Arch:
	     
	22. LANL Project/Shared Parameters used
	☐
	☐
	☐
	     

	
	MEP:
	     
	23. 
	
	
	
	

	
	Struct:
	     
	24. 
	
	
	
	

	13. LANL Browser organization and properly sorted views
	☐
	☐
	☐
	25. 3D views created
	☐
	☐
	☐
	     

	14. Sheet naming convention used
	☐
	☐
	☐
	26. LANL Worksets used/assigned correctly
	☐
	☐
	☐
	     

	15. View naming convention used
	☐
	☐
	☐
	27. LANL Linestyles used
	☐
	☐
	☐
	     

	16. LANL Annotation Symbols used
	☐
	☐
	☐
	28. LANL Lineweights used
	☐
	☐
	☐
	     

	17. LANL Dimension Styles used 
	☐
	☐
	☐
	29. LANL Text Styles used
	☐
	☐
	☐
	     

	18. Linked files provided
	☐
	☐
	☐
	30. Project Base/Survey point coordinate
	☐
	☐
	☐
	     

	19. Any non-LANL elements
	☐
	☐
	☐
	31. LANL View Templates used
	☐
	☐
	☐
	     

	20. Non-permanent views deleted
	☐
	☐
	☐
	32. Any Design Agency updates to templates
	☐
	☐
	☐
	     

	21. Project history schedule filled in
	☐
	☐
	☐
	
	
	
	
	



Comments:
Assessor comments should be black and responses from design team in red.
	



	Project Deliverables Items
	Description

	1. Constructor Name:
	Provide Constructor name

	2. Verify LANL Project BIM QC comments been reconciled
	All comments from the Project BIM QC deliverables have been incorporated and are reflected in the Record BIM

	3. Constructor TIII redlines/Design Agency highlights & initials
	Report on Constructor redlines captured, closed & initials by Design Agency

	4. Record BIM
	Finalized Project BIM with validated incorporation of Redlines, As-builts, LiDAR scans, project data, etc. that capture the final as-constructed facility 3D geometry, location and asset data

	5. TIII PDFs provided
	Set of sheet output from BIM or authoring software in PDF format as well as included PDFs from non-BIM authoring software

	6. -NEW groups provided*
	Extracted final model group -New Record BIM for roll up into Master BIM

	7. Redlines incorporated
	Confirm all redlines have been incorporated in Project BIM before creation of Record BIMs

	8. Design Agency email response stating Project BIM comments were reconciled in documents folder
	Email from Design Agency sent to IPT and copied LANL BIM Manager or VBEO POC verifying Project BIM comments were reconciled. PDF of email saved in documents folder sent in deliverables

	9. Date redlines received
	Provide date of redlines received by Design Agency from Constructor

	10. Standards files provided
	Provide list and files of Standard drawings used to support the project from CAD Standards Manual, Section 300 Drafting Symbols and Conventions

	11. Documents provided: photos, deliverable notifications, PEL files (excel), BIM QC form, etc.
	Provide any additional project files required at each deliverable that are related to Project BIMs either as input, links, or output. This can include the PEL, BIM QC forms, Dynamo scripts, PDFs, photos, etc.

	12. -R Removals groups provided*
	Extracted final model group -R Removal Record BIM for roll up into Master BIM

	Record BIM files
	Description

	13. LANL Browser organization and properly sorted views
	LANL Browser is clean and organized per LANL Revit Templates, LANL Revit Guide 10 – Project Navigation

	14. Sheet naming convention used
	Sheet naming conventions per CAD Standards Manual, Section 200 – CAD Requirements

	15. View naming convention used
	View naming conventions are per LANL Revit Template, LANL Revit Guide 10 – Project Navigation

	16. LANL Annotation Symbols used
	General Annotation Symbols are per LANL Revit Templates, LANL Revit Guide 05 – Annotation General. Discipline specific annotation symbols are per each discipline’s LANL Revit Template Legends

	17. LANL Dimension Styles used
	Dimension Styles in Project BIM are per LANL Revit Template, LANL Revit Guide 06 - Dimensions

	18. Linked files provided
	Provide any linked files within the Record BIMs with deliverables, (.pdf, .dwg, .nwc, .jpg etc.) that support the data integrity of the model and or sheets

	19. Any non-LANL elements
	Provide list of all non-LANL BIM Objects, Revit Families. BIM Object naming follows naming convention of BIM Objects per CAD Standards Manual, Section 400 BIM Standards

	20. Non-permanent views deleted
	Purge all unused and Working views from the Record BIMs

	21. Project history schedule filled in
	Update the Revit Schedule 00 LANL Revit Guide - LANL Master BIM Project History

	22. LANL Project/Shared Parameters used
	Within the Record BIM all parameters that begin with LANL have a value. 

	23. 3D views created
	3D views created reflecting discipline only elements for federated model incorporation

	24. LANL Worksets used/assigned correctly
	Worksets are assigned to the correct Worksets per LANL Revit Templates, LANL Revit Guide 03 – Authoring Content

	25. LANL Linestyles used
	Line Styles in Project BIM are per LANL Revit Template, LANL Revit Guide 08 – Line Styles

	26. LANL Lineweights used
	Line Weights are per LANL Revit Template, LANL Revit Guide 09 – Line Weights

	27. LANL Text Styles used
	Text Styles in Project BIM are per LANL Revit Templates, LANL Revit Guide 07 – Text Styles.

	28. Project Base/Survey point coordinate
	Provide coordinated Project Base point and coordinated Survey Point location

	29. LANL View Templates used
	View Templates are per LANL Revit Templates

	30. Any Design Agency updates to templates
	Provide list of changes or updates to the LANL Revit Templates that will support and or enhance the use of the LANL Revit Templates



image1.jpeg
1% Los Alamos

NATIONAL LABORATORY




