|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ASME B31.9 -2014 Valve Comparison (907.1.2)** | | | | | |
|  | Comparable Listed Valve |  | Evaluated Valve |  | Within Limitations? |
| Manufacturer |  |  |  |  |
| Model |  |  |  |  |
| Pressure Rating |  |  |  |  |  |
| Temperature Rating |  |  |  |  |  |
| Service |  |  |  |  |  |
| Composition |  |  |  |  |  |
| Mechanical Properties |  |  |  |  |  |
| Dimensions |  |  |  |  |  |
| Method of Manufacture |  |  |  |  |  |
| Quality Control Standard |  |  |  |  |  |

**Conclusion**:

In Accordance with ASME B31.9-2014, Paragraph 907.1.2, these valves are being used in accordance with the manufacturer's temperature and pressure ratings of

Attach documentation if necessary to support the above information.

|  |  |  |  |
| --- | --- | --- | --- |
| Evaluated By: |  | Date: |  |
| CPSO/SMPO Designee: |  | Date: |  |